
Mode 1 - No memory lock features enabled
Mode 1 - SPM and LPM are allowed in Application section
Mode 2 - SPM is prohibited in the Boot loader section

mc161c = 1
OCDEN = 0
JTAGEN = 0
SPIEN = 0
WDTON = 1
EESAVE = 1
CKDIV8 = 1
CKOUT = 1

BOOTTRST = 0
BOOTSZ = 01

BODLEVEL=111

CKSEL=111 Ext. crystal osc. 8MHz, start-up time: 16K CK + 65 ms
SUT=11